**RV Campsite Setup & Operating Tips**

**2020 Winnebago Outlook 22C**

**Setup**

* All hookups and hoses are on the driver side, back into your site for easy set up.
* Most campsites have leveled parking pads, but you may need the leveling blocks.
* This Outlook doesn’t have a leveling system.
* Check next to the RV for awning clearance
* Lay out the rug in front of the door, set up your chairs, picnic tablecloth, etc.

**Utilities**

* Electric
* Make sure the breaker switch is off on the campsite’s power pedestal. Plug in, then flip the breaker on.
* Use the surge protector when plugging into the electric hookup (The outlook is a 30 amp rig but we have an adaptor if 50 amp is all that’s available at your campsite).
* If you’re at a home (with regular 20 amp power outlets) you can plug into electricity but you **CAN’T run the AC** in the RV. You can still use lights and microwave.
* Water
* Connect the white hose (with pressure regulator & filter).
* We keep the water tank in the rig about 2/3 full, for flushing and sink usage while you are driving. Not too full or it will weigh down the rig.
* Propane is on, your stove top and water heater are ready to go
* Water pump *and* water heater need to be on to warm up your water.
* Sewer
* Hoses have been cleaned, but grab your gloves for extra sanitation
* Connect the black hose, use the sloped support for best drainage.
* Black water tank (toilet stuff) **always keep black water valve closed**, until you’re ready to dump.
* Grey water tank (shower & sink) can be left open at campsite to allow soapy water to freely run into sewer, but the day before you dump you’ll close the grey water valve and allow water to fill the grey water tank. This will create some pressure to clean the black tank when you’re ready to leave.
* **Helpful Tip:** Turn off the bathroom fan and close the vent before you flush. An open vent will cause an updraft, sucking the odors from the black tank into the air.
* **4 minute utility hookup youtube video: https://rb.gy/admdgy**
* **4 minute grey/black water dump video: https://rb.gy/yoaqbk**

**Departure**

* Dump/clean sewer hookup
* It’s easiest to empty the tanks when you’re fully hooked up at the site (versus waiting in line at a dump station and feeling rushed if it’s busy, and there might not be a water hose)
* Empty black tank first
* Next, empty gray water, the soapy water helps clean out the hose
* Black Tank Flush with the water hose
* Drain sewer hose, spray end caps with disinfectant and put away
* Make sure the grey and black valves are closed
* Use hose & soap to wash off hands, or toss your gloves, hand sanitizer is handy!

**Refrigerator**

* The fridge operates off of the 120-volt electrical system. In order to operate, the refrigerator requires either the shoreline to be plugged in, the generator running, or inverter power. The inverter is intended to power the refrigerator **when driving.** The house batteries will drain quickly if the refrigerator is powered from the inverter when the engine is not running.
* The fridge/freezer will cool while you’re driving to your site (make sure inverter **switch is on** while driving). Then it will run on electricity when you’re hooked up at the campsite.

**When you’re driving:**

* The sink & toilet can be used while the RV being driven.
* Just turn the water pump on (panel located to the right of the microwave).
* Flip it back off when you’re done using the water
* If you want to use electricity (microwave, TV, AC, outlets) in the cabin while driving - you’ll need to turn on the generator (hold down for 3-5 seconds to turn on, press off when you’re done)
* The USB ports under the dinette should be able to charge while driving. The other outlets in the back cabin won’t charge while driving.
* If you use the toilet/sinks between the campsite and return, find a dump station and empty tanks **before returning the RV to us.**

Have the best time & text/call with any questions!

**Contact Info:**

Jared McAdams 405-412-6374

Amy McAdams 405-627-0390